|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Name of Safe Job Procedure** | **Roof Cutter** | | | | **SJP #** | | 00-0\_\_ |
| **Hazard Rating:** |  | High |  | Moderate | |  | Low |
| **Date Developed:** | Enter Date Here | | | | **Revision Date:** | | Enter Date Here |
| **Reviewed by:**(name & title) | Add name of Management representative | | | | **Date:** | | Enter Date Here |
| **Reviewed by:** (name & title) | Add name of worker representative. | | | | **Date:** | | Enter Date Here |

**Instructions:**

* Management and Worker representatives must review this safe job procedure (SJP) prior to implementation, annually, or any time the task, equipment, or materials change.
* Do NOT perform this procedure until you have been appropriately trained and authorized to do so by your supervisor.

|  |
| --- |
| **Required Training:**   * Only trained operators to operate |

**Required PPE:**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| Eye Protection | Face-Shield | Safety Footwear | Hearing Protection | Type of Gloves | Hard Hat | Protective Clothing | No Loose clothing, jewelry |

|  |
| --- |
| **Potential Hazards:**  **Flying debris**   * Ensure cutting pathway is delineated * Cut away from other workers   **Noise**   * Wear hearing protection while cutter is in operation |
| **Pre-Task Safety Checks**   * Pre-use equipment inspection ensuring guards are in place * Check cutting area for buried utilities or other blind hazards * Ensure travel path is clear, free from obstacles and other workers |
| **Job Steps**   1. Start the roof cutter. 2. Adjust the roof cutter depth setting. 3. Slowly start to cut the roof system. Always be aware of hazards on the roof. 4. When complete, shut the roof cutter off. 5. Move the roof cutter away from the work area. |