|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Name of Safe Job Procedure** | **Temporary Guardrail Installation** | | | | **SJP #** | | 00-0\_\_ |
| **Hazard Rating:** |  | High |  | Moderate | |  | Low |
| **Date Developed:** | Enter Date Here | | | | **Revision Date:** | | Enter Date Here |
| **Reviewed by:**(name & title) | Add name of Management representative | | | | **Date:** | | Enter Date Here |
| **Reviewed by:** (name & title) | Add name of worker representative. | | | | **Date:** | | Enter Date Here |

**Instructions:**

* Management and Worker representatives must review this safe job procedure (SJP) prior to implementation, annually, or any time the task, equipment, or materials change.
* Do NOT perform this procedure until you have been appropriately trained and authorized to do so by your supervisor.

|  |
| --- |
| **Required Training:**   * Fall Protection certification |

**Required PPE:**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| Eye Protection | Face-Shield | Safety Footwear | Hearing Protection | Type of Gloves | Hard Hat | Protective Clothing | No Loose clothing, jewelry |

|  |
| --- |
| **Potential Hazards:**  **Fall from height**   * Pre-use inspection for equipment * Select an anchor with sufficient strength * Use fall restraint, not fall arrest, whenever possible |
| **Pre-Task Safety Checks**   * Perform pre-use inspection on all equipment and anchors * Inspect all clamps/ handrail brackets |
| **Job Steps**   1. Select an anchor point for the travel restraint system. 2. Attach rope lanyard to the anchor. 3. Connect the harness to the anchored rope. 4. Carefully walk to the roof edge, maintaining fall restraint lanyard length. 5. Install a parapet clamp or guardrail bracket. 6. Insert uprights into the parapet clamp or bracket. 7. Install guard rails in uprights. |